REMOVAL ■ CAUTION ■ Use shop cloths to protect parts from damage during removal and installation.

1.Operate the seat control switch knob to move the seat slide to the rearmost position.

2.Remove the front slide cover.

(1)Front outer slide cover

| : Pawl

(2)Front inner slide cover

| : Pawl

3.Remove the mounting bolts from the front seat front side.

4.Operate the seat control switch knob to move the seat slide to the foremost position.

5.Remove the rear slide outer and inner covers.

| : Pawl

6.Remove the rear inner bolt cap (Driver seat only).

7.Remove the mounting bolts from the front seat rear side.

8.Set the seatback vertically.

9.Lift up the seat cushion front side, and disconnect the harness connector under the seat cushion and remove the harness clamp.
■ CAUTION ■
For the seat with side air bag, disconnect the battery cable from the negative terminal after checking that the ignition switch is OFF, wait for at least 3 minutes, and then disconnect the connector.

10.Remove the front seat from the vehicle.
■ CAUTION ■

- Use shop cloths to protect parts from damage during removal and installation.
- Two people must perform removal and installation of the seat assembly to prevent damage or to keep from dropping it.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Always fix the harness clamp in the normal position.

- Be careful that only driver seat rear inner mounting bolt is different from others among the front seat mounting bolts.