1.PERFORM ACTIVE TEST With CONSULT-III

1. Connect the E-SUS control unit harness connector and front LH shock absorber actuator harness connector.
2. Select “SHOCK ABSORBER ACTUATOR” in “ACTIVE TEST”.
3. On the display, change the “Operation half cycle”, and check that the operation noise is heard from the actuator.

   Test item | Display Item | Display
   Operation half cycle
   SHOCK ABSORBER ACTUATOR | FRONT LEFT ACTUATOR | 0.1 seconds – 1 second (cycle in 0.1 seconds)

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the front LH shock absorber. Refer to Removal and Installation (GT-R certified NISSAN dealer).