Measurement Dimensions marked with ″*″ indicate symmetrically identical dimensions on both the right and left hand of the vehicle.

Unit: mm (in)

«The others»

Unit: mm (in)
| Point | Dimension | Memo |  | Point | Dimension | Memo |  | Point | Dimension | Memo |
| G - g | 902.2 (35.520) |  |  |  |  |  |  |  |  |  |

Measurement Points

| : Vehicle front |  |  |  |

Unit: mm (in)
Point | Remarks | Point | Remarks
A, a | Upper dash positioning mark | E, e | Radiator core support mounting installing hole center φ14 (0.55)
B, b | Hood hinge installing hole center φ10 (0.39) | F, f | Front side member location hole center φ20 (0.79)
C, c | Front strut installing hole center φ8.5 (0.335) | G, g | Front strut housing upper link installing hole center φ12.5 (0.492)
D, d | Front fender installing hole center φ12 (0.47) | H, h | Bumper reinforcement mounting installing hole center φ10 (0.39)