Work after hoodledge reinforcement, rear fender, and lock pillar reinforcement are removed. Remove the front pillar brace (reusable).

1. | Outer sill brace | 2. | Urethane foam | 3. | Body sealing
Unit: mm (in) |  |  |  |
: Vehicle front : Weld the parts onto the back of the component part.
Replacement parts
• | Outer sill reinforcement (LH) |  |  |  |

View C: Before installing front pillar brace

1. | Urethane foam |  |  |  |
Unit: mm (in) |  |  |  |
: Vehicle front

View H: Before installing outer sill reinforcement