Suppresses the deployment of front passenger air bag when the condition of passenger seat is empty or occupied with a child and child-seat. Also illuminates front passenger air bag OFF indicator lamp when the condition of passenger seat is occupied with a child-seat and child. In case of malfunction the blinking of the air bag warning lamp reports the malfunction to driver, and by the on board self-diagnosis system or CONSULT-III can detect the cause.
OPERATION
Illuminates front passenger air bag OFF indicator when the passenger seat is empty or occupied by a child or a child-seat.
STRUCTURE
Front passenger air bag OFF indicator with LED illumination.
INSTALLATION
Front passenger air bag OFF indicator is installed at the instrument panel center.