DESCRIPTION The following figure shows the areas that are sealed at the factory. Sealant that is applied to these areas should be smooth and free from cuts or gaps. Care should be taken not to apply an excess amount of sealant and not to allow other unaffected parts to come into contact with the sealant.

| : Vehicle front |  |  |  |
| : Sealed portions |  |  |  |

| : Vehicle front |  |  |  |
| : Sealed portions |  |  |  |

| : Vehicle front |  |  |  |
| : Sealed portions |  |  |  |