■ CAUTION ■ Check vehicle is empty when lifting.

- The board-on lift attachment (A) set at front end of vehicle should be set on the front of the jack point under the door opening.
- Position attachments at front and rear ends of board-on lift.

  | : Vehicle front

- Be careful to use lift attachment (A) that has contact surface (b) for 90mm (3.5 in) or less. Always set lift attachment to the lift up point (3) center, so that it does not touch side sill (1) and under cover (2).