1.CHECK INTAKE SENSOR

1. Turn the ignition switch OFF.
2. Disconnect the intake sensor connector. Refer to Exploded View (GT-R certified NISSAN dealer).
3. Check the resistance between the intake sensor terminals. Refer to the applicable table for the normal value.

   Terminal | Condition | Resistance: kΩ
   Temperature: °C (°F)
   1 | 2 | −15 (5) | 12.84
   −10 (14) | 10.02
   −5 (23) | 7.89
   0 (32) | 6.27
   5 (41) | 5.02
   10 (50) | 4.06
   15 (59) | 3.30
   20 (68) | 2.70
   25 (77) | 2.23
   30 (86) | 1.85
   35 (95) | 1.54
   40 (104) | 1.30
   45 (113) | 1.09

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the intake sensor.