REMOVAL Driver Side

1.Remove heater & cooling unit assembly. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Remove aspirator.

3.Remove mounting screws (A), and then remove heater pipe cover (1).

4.Remove mounting screws (B), and then remove foot duct LH (2).

Passenger Side

1.Set the temperature (passenger side) at 18.0°C (60°F).

2.Disconnect the battery cable from negative terminal.
■ CAUTION ■
The angle may be out, when installing the air mix door motor to the air mix door, unless the above 2 procedures are performed.

3.Remove heater & cooling unit assembly. Refer to Exploded View (GT-R certified NISSAN dealer).

4.Remove air mix door motor (passenger side). Refer to Exploded View.

5.Remove mode door motor and links. Refer to Exploded View.

6.Remove mounting screws (A), and then remove evaporator cover (1).

7.Remove mounting screws (B), and then remove foot duct RH (2).

INSTALLATION
Installation is basically the reverse order of removal.