DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0715 | Input/turbine speed sensor "A" circuit | A DTC is set if the status 1 or 2 below is detected with sleeve A1 or A2 engaged in an even gear.

1. The difference between the actual output shaft speed and the output shaft speed converted from the clutch A speed is 1,000 rpm or more.
2. The difference between the vehicle speed signal (meter) (CAN signal) and the output shaft speed converted from the clutch A speed is 1,000 rpm or more.

- Clutch A speed sensor
- Sleeve A1 related part
- Sleeve A2 related part
- Harness or connector
  (Open or short in the clutch A speed sensor circuit)

DTC CONFIRMATION PROCEDURE
■ CAUTION ■
Be careful of the driving speed.
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE (PART 1)
With CONSULT-III

1. Start the engine.
2. Select “RANGE”, “GEAR” and “ENGINE SPEED” in “Data Monitor”.
3. Run the vehicle and maintain the following conditions for 5 seconds or more.

   RANGE | : M
   GEAR | : 4
   ENGINE SPEED | : 1,500 rpm or more

4. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Run the vehicle and maintain the following conditions for 5 seconds or more.

   Shift lever | : M range
   Gear | : 4
   Engine speed | : 1,500 rpm or more

3. Check self-diagnosis.

Is DTC P0715 detected?
YES>>Go to Diagnosis Procedure (NHPC).
NO>>GO TO 3.
3.PERFORM DTC CONFIRMATION PROCEDURE (PART 2)
With CONSULT-III

1. Select “RANGE”, “GEAR” and “VEHICLE SPEED” in “Data Monitor”.
2. Run the vehicle and maintain the following conditions for 5 seconds or more.

   RANGE | : M
   GEAR | : 6
   VEHICLE SPEED | : 36 – 44 km/h (23 – 27 MPH)

3. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Run the vehicle and maintain the following conditions for 5 seconds or more.

   Shift lever | : M range
   Gear | : 6
   Vehicle speed | : 36 – 44 km/h (23 – 27 MPH)

3. Check self-diagnosis.

Is DTC P0715 detected?
YES>>Go to Diagnosis Procedure (NHPC).
NO>>Go to Intermittent Incident.