1.PERFORM INITIALIZATION Perform initialization with CONSULT-III. Reregister all Intelligent Keys. For initialization and registration of Intelligent Key. Refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”. Can the system be initialized and can the engine be started with reregistered Intelligent Key?
YES>>INSPECTION END
NO>>GO TO 2.
2.REPLACE INTELLIGENT KEY

1. Replace Intelligent Key.
2. Perform initialization with CONSULT-III. For initialization and registration of Intelligent Key. Refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”.

Can the system be initialized and can the engine be started with reregistered Intelligent Key?
YES>>INSPECTION END
NO>>GO TO 3.
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END