1.CHECK TRANSMITTER ID REGISTRATION

1. Perform transmitter ID registration for all wheels. Refer to Transmitter ID Registration Procedure.
2. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
3. Within 5 minutes, use CONSULT-III “DATA MONITOR” to display the tire pressure for all wheels.
4. Check that the displayed tire pressure is the specified value.

   Monitor item | Measuring condition | Displayed value
   AIR PRESS FL | Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes. | Internal pressure of tires
   AIR PRESS FR
   AIR PRESS RR
   AIR PRESS RL

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.CHECK TRANSMITTERS

1. Perform trouble diagnosis for the transmitter. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
2. Perform transmitter ID registration for all wheels. Refer to Transmitter ID Registration Procedure.
3. Check that transmitter ID registration is completed for all wheels.

Is transmitter ID registration for all wheels been completed?
YES>>INSPECTION END
NO>>Replace the transmitter.