INSPECTION Brake Pedal Height Check the height between the dash lower panel (1) and the top face of the brake pedal (H1).

H1 | : Refer to Brake Pedal.

■ CAUTION ■
Perform it with the floor trim removed.
ASCD Brake Switch and Stop Lamp Switch
Check the clearance (C) between the stopper rubber (1) and the tip of the ASCD brake switch and stop lamp switch (2) unit.

C | : Refer to Brake Pedal.

■ CAUTION ■
The stop lamp must turn off when the brake pedal is released.
Brake Pedal Play
Press the brake pedal (pad), check the brake pedal play (A) (dimension until the fluid pressure occurs).

A | : Refer to Brake Pedal.

Depressed Brake Pedal Height
Check the height between the dash lower panel (1) and the top face of the brake pedal (H2) when depressing the brake pedal with a force of 490 N (50 kg, 110lb) while the engine is running.

H2 | : Refer to Brake Pedal.

■ CAUTION ■
Perform it with the floor trim removed.
ADJUSTMENT
Brake Pedal Height

1.Disconnect the ASCD brake switch and stop lamp switch connector.

2.Loosen the ASCD brake switch and stop lamp switch by turning it 45° counterclockwise.

3.Adjust the brake pedal height with the following procedure.

(1)Loosen the lock nut (1) of the input rod.
■ CAUTION ■
The threaded end (2) of the input rod must project to the inner side (L) of the clevis (3).

(2)Rotate the input rod, adjust the brake pedal to the specified height (H1).

H1 | : Refer to Brake Pedal.

(3)Tighten the lock nut. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■
The threaded end (2) of the input rod must project to the inner side (L) of the clevis (3).

4.Adjust the clearance between the stopper rubber and the tip of ASCD brake pedal and stop lamp switch unit after adjusting the brake pedal height.

ASCD Brake Switch and Stop lamp Switch (Brake Pedal Play)

1.Disconnect the ASCD brake switch and stop lamp switch connector.

2.Loosen the ASCD brake switch and stop lamp switch by turning it 45° counterclockwise.

3.Press the ASCD brake switch and stop lamp switch (2) until the tip of the unit contacts with the stopper rubber (1).
■ CAUTION ■

- The clearance (C) between the stopper rubber and the tip of ASCD brake switch and stop lamp switch unit must be within the specified value.

  C | : Refer to Brake Pedal.

- The stop lamp must turn off when the brake pedal is released.