1.Perform “Data Monitor” of CONSULT-III to check for any malfunctioning item.

2.Check the malfunction combinations.

Malfunction item: ×
Malfunction combination | Data monitor item
FR WIPER HI | FR WIPER LOW | FR WASHER SW | FR WIPER INT | INT VOLUME | TURN SIGNAL R | TURN SIGNAL L | TAIL LAMP SW | HI BEAM SW | HEAD LAMP SW 1 | HEAD LAMP SW 2 | AUTO LIGHT SW | PASSING SW
A |  | × | × |  |  | × | × |  |  |  |  |  |
B | × |  |  | × |  |  |  |  |  | × |  |  | ×
C |  |  |  |  | × |  |  |  | × |  | × |  |
D |  |  |  |  | × |  |  | × |  |  |  | × |
E |  |  |  |  | × |  |  |  |  |  |  |  |
F | × |  |  |  | × |  |  |  |  |  |  |  |
G |  |  | × |  | × |  |  |  |  |  |  |  |
H |  | × |  | × |  |  |  |  |  |  |  | × |
I |  |  |  |  |  |  | × |  |  |  | × |  | ×
J |  |  |  |  |  | × |  | × | × | × |  |  |
K | All Items
L | If only one item is detected or the item is not applicable to the combinations A to K

3.Identify the malfunctioning part from the agreed combination and repair or replace the part.

Malfunction combination | Malfunctioning part | Repair or replace
A | Combination switch INPUT 1 circuit | Inspect the combination switch input circuit applicable to the malfunctioning part. Refer to Diagnosis Procedure.
B | Combination switch INPUT 2 circuit
C | Combination switch INPUT 3 circuit
D | Combination switch INPUT 4 circuit
E | Combination switch INPUT 5 circuit
F | Combination switch OUTPUT 1 circuit | Inspect the combination switch output circuit applicable to the malfunctioning part. Refer to Diagnosis Procedure.
G | Combination switch OUTPUT 2 circuit
H | Combination switch OUTPUT 3 circuit
I | Combination switch OUTPUT 4 circuit
J | Combination switch OUTPUT 5 circuit
K | BCM | Replace BCM. Refer to Exploded View.
L | Combination switch | Replace the combination switch.