1.CHECK THROTTLE POSITION SENSOR

1. Turn ignition switch OFF.
2. Reconnect all harness connectors disconnected.
3. Perform Special Repair Requirement (GT-R certified NISSAN dealer).
4. Turn ignition switch ON.
5. Set selector lever to A position.
6. Check the voltage between ECM harness connector terminals under the following conditions.

   ECM | Condition | Voltage (V)
   Connector | + | –
   Terminal | Terminal
   F101 | 40 [TP sensor 1 (bank 1)] | 20 | Accelerator pedal : Fully released | More than 0.36
   Accelerator pedal : Fully depressed | Less than 4.75
   28 [TP sensor 1 (bank 2)] | 15 | Accelerator pedal : Fully released | More than 0.36
   Accelerator pedal : Fully depressed | Less than 4.75
   36 [TP sensor 2 (bank 1)] | 20 | Accelerator pedal : Fully released | Less than 4.75
   Accelerator pedal : Fully depressed | More than 0.36
   32 [TP sensor 2 (bank 2)] | 15 | Accelerator pedal : Fully released | Less than 4.75
   Accelerator pedal : Fully depressed | More than 0.36

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.REPLACE ELECTRIC THROTTLE CONTROL ACTUATOR

1. Replace malfunctioning electric throttle control actuator.
2. Go to Special Repair Requirement (GT-R certified NISSAN dealer).

>>INSPECTION END