1.CHECK LICENSE PLATE LAMP BULB Check the applicable lamp bulb. Is the bulb normal? YES>>GO TO 2. NO>>Replace the bulb.
2.CHECK LICENSE PLATE LAMP OPEN CIRCUIT

1. Turn the ignition switch OFF.
2. Disconnect IPDM E/R connector and the license plate lamp connector.
3. Check continuity between the IPDM E/R harness connector and the license plate lamp harness connector.

   IPDM E/R | License plate lamp | Continuity
   Connector | Terminal | Connector | Terminal
   RH | E5 | 7 | B154 | 1 | Existed
   LH | B152 | 1

Does continuity exist?
YES>>GO TO 3.
NO>>Repair the harnesses or connectors.
3.CHECK LICENSE PLATE LAMP GROUND OPEN CIRCUIT
Check continuity between the license plate lamp harness connector and the ground.

License plate lamp | Ground | Continuity
Connector | Terminal
RH | B154 | 2 | Existed
LH | B152 | 2

Does continuity exist?
YES>>Replace the license plate lamp.
NO>>Repair the harnesses or connectors.