COMMUNICATION LINE

- Solder the repaired area and wrap tape around the soldered area.
  NOTE：
  A fray of twisted lines must be within 110 mm (4.33 in).
- Bypass connection is never allowed at the repaired area.
  NOTE：
  Bypass connection may cause communication error as spliced wires that are separate from the main line or twisted lines lose noise immunity.
- Replace the applicable harness as an assembly if error is detected on the shield lines of communication line.