DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0706 | Transmission range sensor "A" circuit range/performance | A DTC is set if any of the following sensors and switch is/are stuck to ON or OFF consecutively: Range sensors No. 0, No. 1, No. 2, No. 3, No. 4 or No. 5, and park position switch. |

- Range sensor
- Park position switch
- Harness or connector
  (Open or shorted in the range sensor circuit)
  (Open or shorted in the park position switch circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine.
2. Shift the shift lever as per the following: P→R→N→A positions (Keep the shift lever for 5 seconds or more at each position).
3. Shift the shift lever as per the following: A→N→R→P positions (Keep the shift lever for 5 seconds or more at each position).
4. Repeat the procedure shown in 2 and 3 above 2 times.
5. Check “Self Diagnostic Result” of “TRANSMISSION”.

Is DTC P0706 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.