1.CHECK “LO- BATT OF KEY FOB WARN” SETTING IN “WORK SUPPORT” Check “LO- BATT OF KEY FOB WARN” setting in “WORK SUPPORT”. Refer to CONSULT-III Function (BCM - INTELLIGENT KEY). Is the inspection result normal? YES>>GO TO 2.
NO>>Set “LO- BATT OF KEY FOB WARN” setting in “WORK SUPPORT”.
2.CHECK INTELLIGENT KEY
Check Intelligent key.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK COMBINATION METER DISPLAY FUNCTION
Check combination meter display function.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.CHECK INSIDE KEY ANTENNA
Check inside key antenna.

- Instrument center: Refer to DTC Logic.
- Console: Refer to DTC Logic.
- Trunk room: Refer to DTC Logic.

Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.