1.CHECK DOOR LOCK FUNCTION Lock/unlock door with door request switch. Refer to System Description. Is the operation normal? YES>>GO TO 2.
NO>>Check door lock function. Refer to Diagnosis Procedure.
2.PERFORM WORK SUPPORT
Perform “INSIDE ANT DIAGNOSIS” on “Work Support” of “INTELIGENT KEY”.
Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
>>GO TO 3.
3.PERFORM SELF DIAGNOSTIC RESULT
Perform Self Diagnostic result of “INTELIGENT KEY”.
Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
Is DTC detected?
YES>>Refer to DTC Logic (instrument center), refer to DTC Logic (console), refer to DTC Logic (trunk room).
NO>>GO TO 4.
4.CHECK PUSH-BUTTON IGNITION SWITCH
Check push-button ignition switch.
Refer to Component Function Check.
Is the inspection normal?
YES>>GO TO 5.
NO>>Repair or replace malfunctioning parts.
5.CONFIRM THE OPERATION
Confirm the operation again.
Is the inspection normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.