1.CHECK BUZZER (COMBINATION METER) Check buzzer (combination meter). Refer to Component Function Check. Is the inspection result normal? YES>>GO TO 2.
NO>>Repair or replace the malfunctioning parts.
2.CHECK DOOR SWITCH
Check door switch (driver side).
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK KEY SLOT
Check key slot.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.CHECK COMBINATION METER DISPLAY FUNCTION
Check combination meter display function.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CHECK KEY SLOT INDICATOR
Check key slot indicator.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 6.
NO>>Repair or replace the malfunctioning parts.
6.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.