1.CHECK ACCELERATOR PEDAL POSITION SENSOR

1. Turn ignition switch OFF.
2. Reconnect all harness connectors disconnected.
3. Turn ignition switch ON.
4. Check the voltage ECM harness connector terminals under the following conditions.

   ECM | Condition | Voltage (V)
   Connector | + | –
   Terminal | Terminal
   M107 | 104 (APP sensor 1) | 103 | Accelerator pedal | Fully released | 0.5 - 1.0
   Fully depressed | 4.2 - 4.8
   108 (APP sensor 2) | 107 | Fully released | 0.25 - 0.50
   Fully depressed | 2.0 - 2.5

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.REPLACE ACCELERATOR PEDAL ASSEMBLY

1. Replace accelerator pedal assembly.
2. Go to Special Repair Requirement (GT-R certified NISSAN dealer).

>>INSPECTION END