- Since vehicle specifications are not included in the AV control unit after replacement, it is required to write vehicle specifications with CONSULT‐III.
- Configuration has three functions as follows.

  Function | Description
  READ CONFIGURATION |
  - Reads the vehicle configuration of current AV control unit.
  - Saves the read vehicle configuration.
  WRITE CONFIGURATION‐Manual selection | Writes the vehicle configuration with manual selection.
  WRITE CONFIGURATION‐Config file | Writes the vehicle configuration with saved data.