■ CAUTION ■ Disconnect the battery negative terminal or remove the fuse. REMOVAL

1.Insert any appropriate tool (A) into the gap between the side turn signal lamp and fender protector.

2.Pull the side turn signal lamp toward vehicle outside while pushing metal clip (B) toward vehicle front, and then remove side turn signal lamp from vehicle.

| : Vehicle front

3.Disconnect the side turn signal lamp connector.Remove the side turn signal lamp.

NOTE：
Support the vehicle-side harness of the side turn signal lamp with tape so that it does not drop inside the front fender.
INSTALLATION

1.Connect the side turn signal lamp connector.

2.Fix the pawl side. And then push the clip side.