DTC DETECTION LOGIC NOTE：

- If DTC P0461 is displayed with DTC UXXXX, first perform the trouble diagnosis for DTC UXXXX.
- If DTC P0461 is displayed with DTC P0607, first perform the trouble diagnosis for DTC P0607. Refer to DTC Logic (GT-R certified NISSAN dealer).

Driving long distances naturally affect fuel gauge level.
This diagnosis detects the fuel gauge malfunction of the gauge not moving even after a long distance has been driven.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
P0461 | Fuel level sensor circuit range/performance | The output signal of the fuel level sensor does not change within the specified range even though the vehicle has been driven a long distance. |

- Harness or connectors
  (The CAN communication line is open or shorted)
- Harness or connectors
  (The sensor circuit is open or shorted)
- Combination meter
- Fuel level sensor

DTC CONFIRMATION PROCEDURE
1.PERFORM COMPONENT FUNCTION CHECK
Perform component function check. Refer to Component Function Check (GT-R certified NISSAN dealer).
Use component function check to check the overall function of the fuel level sensor. During this check, a 1st trip DTC might not be confirmed.
Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).