REMOVAL

1.Remove low‐pressure pipe 1 and high‐pressure pipe 3. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■
Cap or wrap the joint of the cooler piping with suitable material such as vinyl tape to avoid the entry of air.

2.Disconnect intake sensor connector.

3.Slide evaporator (1) to passenger side, and then remove evaporator from heater & cooling unit assembly.

4.Remove intake sensor from evaporator.

INSTALLATION
Installation is basically the reverse order of removal.
■ CAUTION ■

- Replace O‐rings with new ones. Then apply compressor oil to them when installing.
- Mark the mounting position of intake sensor bracket prior to removal so that the reinstalled sensor can be located in the same position.
- Female‐side piping connection is thin and easy to deform. Slowly insert the male‐side piping straight in axial direction.
- Insert piping securely until a click is heard.
- After piping connection is completed, pull male‐side piping by hand to make sure that connection does not come loose.
- Check for leakages when recharging refrigerant.