Unit | Description
Combination meter | Receives a buzzer output signal from the BCM and sounds the buzzer.
BCM |

- The BCM receives shift position signal from TCM via CAN communication.
- The BCM detects reverse warning based on the received signal and transmits the buzzer output signal to combination meter via CAN communication.

TCM | Transmits the shift position signal to BCM via CAN communication.