MOUNTING INSPECTION Check the mounting conditions (looseness, backlash) of each component and component conditions (wear, damage) are normal. BALL JOINT AXIAL END PLAY

1.Set front wheels in a straight-ahead position.

2.Place an iron bar or equivalent between front lower link, rear lower link radius rod or suspension arm and axle housing.

3.Measure axial end play by playing it up and down.

Axial end play | : Refer to Ball Joint (GT-R certified NISSAN dealer).

■ CAUTION ■

- Never depress brake pedal when measuring.
- Never perform with tires on level ground.
- Be careful not to damage ball joint boot. never damage the installation position by applying excessive force.

SHOCK ABSORBER
Check for oil leakage and damage. Replace it if necessary.