DISASSEMBLY

1.Remove the front wiper linkage 1 and 2 from the front wiper drive assembly.
■ CAUTION ■
Never bend the linkage or damage the plastic part of the ball joint when removing the wiper linkage.

2.Remove the front wiper motor mounting screws, and then remove the front wiper motor from the front wiper frame.

ASSEMBLY

1.Connect the front wiper motor connector.

2.Operate the front wiper to move it to the auto stop position.

3.Disconnect the front wiper motor connector.

4.Install the front wiper motor to the front wiper frame.

5.Install the front wiper linkage 2 to the front wiper motor and the front wiper frame.

6.Install the front wiper linkage 1 to the front wiper frame.
■ CAUTION ■

- Never drop front wiper motor or cause it to come into contact with other parts.
- Be careful for the grease condition at the front wiper motor and front wiper linkage joint (retainer). Apply Multi−purpose grease or an equivalent if necessary.