Apply the fusible insulator (melsheet) to the floor upper surface and dashboard panel interior side to block noise, vibration, and exhaust gas heat. Use the fusible insulators (A) - (D) for the front floor set as the service parts. Place these parts in the positions shown in the figure, heat these parts by halogen heaters, etc., and then fix the fusible insulators to the floor.

A. | T=2.0 mm (0.08 in) | B. | T=2.0 mm (0.08 in) | C. | T=2.0 mm (0.08 in)
D. | T=2.0 mm (0.08 in) | E. | T=3.0 mm (0.12 in) | F. | T = 3.0 mm (0.12 in) LH and RH are symmetrical.
: Fusible insulator applying part

■ CAUTION ■
Select the fusible insulators (E) and (F) used for the rear floor panel from among the commercial service tool shown in the following table, and then cut and paste them.

Pressure-sensitive insulator
Unit: mm (in)
Part number | Size
G5930-89904 | 500 × 1000 × 1.5T (19.69 × 39.37 × 0.059T)
G5930-89905 | 500 × 1000 × 3.0T (19.69 × 39.37 × 0.118T)
G5930-89906 | 500 × 1000 × 6.0T (19.69 × 39.37 × 0.236T)