1.CHECK TURBOCHARGER BOOST CONTROL SOLENOID VALVE

1. Turn ignition switch OFF
2. Disconnect turbocharger boost control solenoid valve harness connector.
3. Disconnect hoses connected to turbocharger boost control solenoid valve.
4. Check air passage continuity of turbocharger boost control solenoid valve under the following conditions.

   Condition | Air passage continuity between (A) and (B) | Air passage continuity between (A) and (C)
   12 V direct current supply between terminals 1 and 2 | Existed | Not existed
   No supply | Not existed | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace turbocharger boost control solenoid valve.