■ CAUTION ■

- Disconnect the battery negative terminal or remove the fuse.
- After installing the bulb, install the resin cap and the bulb socket securely for watertightness.
- Never touch the glass of bulb directly by hand. Keep grease and other oily matters away from it.
- Never touch bulb by hand while it is lit or right after being turned off.
- Never leave bulb out of lamp reflector for a long time because dust, ,moisture smoke, etc. may affect the performance of lamp. When replacing bulb, be sure to replace it with new one.

HEADLAMP BULB (LO)

1.Remove the front tire. Refer to Exploded View.

2.Remove the fender protector. Keep a service area. Refer to Exploded View.

3.Rotate the resin cap counterclockwise and unlock it.

4.Rotate the bulb socket counterclockwise and unlock it.

5.Remove the retaining spring lock. Remove the bulb from the headlamp housing assembly.
■ CAUTION ■
Never break the xenon bulb ceramic tube when replacing the bulb.

HEADLAMP BULB (HI)

1.Remove the front tire. Refer to Exploded View.

2.Remove the fender protector. Keep a service area. Refer to Exploded View.

3.Remove the washer tank inlet. Refer to Exploded View.*: When replace a left.

4.Rotate the resin cap counterclockwise and unlock it.

5.Disconnect the headlamp bulb (HI) connector.

6.Rotate the bulb socket counterclockwise and unlock it.

7.Remove the bulb from the headlamp housing assembly.

PARKING LAMP BULB

1.Rotate the bulb socket counterclockwise and unlock it.

2.Remove the bulb from the bulb socket.

FRONT TURN SIGNAL LAMP BULB

1.Remove the front tire. Refer to Exploded View.

2.Remove the fender protector. Keep a service area. Refer to Exploded View.

3.Rotate the bulb socket counterclockwise and unlock it.

4.Remove the bulb from the bulb socket.