1.CHECK INTELLIGENT KEY WARNING BUZZER

1. Turn ignition switch OFF.
2. Disconnect Intelligent Key warning buzzer connector.
3. Connect battery power supply directly to Intelligent Key warning buzzer terminals and check the operation.

   Terminal | Operation
   Intelligent Key warning buzzer
   (+) | (−)
   1 | 3 | Buzzer sounds

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace Intelligent Key warning buzzer. Refer to Removal and Installation.