■ WARNING ■

- Before servicing, turn ignition switch OFF, disconnect battery negative terminal and wait 3 minutes or more.
- Never use the air tools or electric tools for servicing.

REMOVAL

1.Remove the front seat belt retractor. Refer to Removal and Installation.

2.Disconnect the satellite sensor harness connector.

3.Remove the satellite sensor mounting nut, and then remove the satellite sensor.

■ CAUTION ■

- Never impact the side air bag (satellite) sensor.
- Replace the side air bag (satellite) sensor if it is dropped or sustains an impact.
- Replace the side air bag (satellite) sensor of deployed SRS front side air bag and deployed SRS side curtain air bag.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Never use the old fixing nuts after removal, replace with the new nuts.
- If malfunction is detected by the air bag warning lamp, after repair or replacement of the malfunctioning parts, reset the memory using self-diagnosis or CONSULT-III. Refer to CONSULT-III Function.
- After the work is complete, check that no system malfunction is detected by air bag warning lamp.