■ CAUTION ■ Before performing the diagnosis, check that the following is normal.

- Interior room lamp power supply
- Step lamp bulb

1.CHECK STEP LAMP OPERATION
CONSULT-III ACTIVE TEST

1. Turn the ignition switch ON.
2. Select "STEP LAMP TEST" of BCM (INT LAMP) active test item.
3. With operating the test items, check that step lamps operation.

   On | : Step lamp ON
   Off | : Step lamp OFF

Are the step lamps turned?
YES>>Step lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.