■ CAUTION ■

- Never spill or splash brake fluid on painted surfaces. Brake fluid may seriously damage paint. Wipe it out immediately and wash with water if it gets on a painted surface.
- Turn the ignition switch OFF and disconnect the ABS actuator and electric unit (control unit) connector or the battery negative terminal before performing work.
- Wrap the flare nut wrench with waste cloth to protect the caliper from damage.
- If the brake fluid adheres to the caliper or disc rotor, quickly wipe it out.
- Never allow foreign matter (e.g. dust) and oils other than brake fluid to enter the reservoir tank.
- Since brake fluid is susceptible to deterioration from moisture, discard brake fluid remaining in the container.

1.Check that there is no foreign material in the reservoir tank, and refill the brake fluid with new one.
■ CAUTION ■
Never reuse drained brake fluid.

2.Loosen the bleeder valve, slowly depress the brake pedal to the full stroke, and then release the pedal. Repeat this operation at intervals of 2 or 3 seconds until all of the brake fluid is discharged. Then close the bleeder valve with the brake pedal depressed. Repeat the same work on each wheel.

3.Perform the air bleeding. Refer to Bleeding Brake System.