- When removing or disassembling each component, be careful not to damage or deform it. If a component may be subject to interference, be sure to protect it with a shop cloth.

- When removing (disengaging) components with a screwdriver or similar tool, be sure to wrap the component with a shop cloth or vinyl tape to protect it.

- Protect the removed parts with a shop cloth and keep them.

- Replace a deformed or damaged clip.

- If a part is specified as a non-reusable part, always replace it with new one.

- Be sure to tighten bolts and nuts securely to the specified torque.

- After re-installation is completed, be sure to check that each part works normally.

- Follow the steps below to clean components.

- Water soluble foul: Dip a soft cloth into lukewarm water, and wring the water out of the cloth to wipe the fouled area.Then rub with a soft and dry cloth.

- Oily foul: Dip a soft cloth into lukewarm water with mild detergent (concentration: within 2 to 3%), and wipe the fouled area.Then dip a cloth into fresh water, and wring the water out of the cloth to wipe the detergent off. Then rub with a soft and dry cloth.

- Do not use organic solvent such as thinner, benzene, alcohol, and gasoline.

- For genuine leather seats, use a genuine leather seat cleaner.