INSPECTION AFTER REMOVAL Check the front suspension member for significant deformation, cracks and damages. Replace if necessary. INSPECTION AFTER INSTALLATION

1.Check wheel sensor harness connector for proper connection. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Check wheel alignment. Refer to Adjustment.

3.Adjust the neutral position of the steering angle sensor. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).