■ WARNING ■

- Before servicing, turn ignition switch OFF, disconnect battery negative terminal and wait 3 minutes or more.
- Never use the air tools or electric tools for servicing.

REMOVAL

1.Remove the crash zone sensor mounting nut.

2.Disconnect the crash zone sensor harness connector, and then remove the crash zone sensor.

■ CAUTION ■

- Never impact the crash zone sensor.
- Replace the crash zone sensor if it is dropped or sustains an impact.
- Replace the crash zone sensor of deployed SRS driver air bag and deployed SRS front passenger air bag.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Never use old fixing nuts after removal, replace with new nuts.
- If malfunction is detected by the air bag warning lamp, after repair or replacement of the malfunctioning parts, reset the memory using self-diagnosis or CONSULT-III. Refer to CONSULT-III Function.
- After the work is complete, check that no system malfunction is detected by air bag warning lamp.