BEFORE REPLACEMENT When replacing BCM, save or print current vehicle specification with CONSULT‐III configuration before replacement. NOTE： If “READ CONFIGURATION” can not be used, use the “WRITE CONFIGURATION - Manual selection” after replacing BCM.
AFTER REPLACEMENT
■ CAUTION ■

- When replacing BCM, you must perform “WRITE CONFIGURATION” with CONSULT‐III.

- Complete the procedure of “WRITE CONFIGURATION” in order.
- If you set incorrect “WRITE CONFIGURATION”, incidents might occur.
- Configuration is different for each vehicle model. Confirm configuration of each vehicle model.

- When replacing BCM, perform the system initialization (NATS).