1.CHECK AXIS A FEED PRESSURE SOLENOID VALVE (PART 1) Check the resistance between transmission unit harness connector terminals.

Transmission unit harness connector | Condition | Resistance (Approx.)
Connector | Terminal
B49 | 14 | 15 | Transmission oil temperature: 20°C (68°F) | 3.8–4.4Ω
Transmission oil temperature: 50°C (122°F) | 4.3–5.0Ω
Transmission oil temperature: 80°C (176°F) | 4.7–5.4Ω

Is the inspection result normal?
YES>>GO TO 2.
NO>>Repair or replace damaged parts.
2.CHECK AXIS A FEED PRESSURE SOLENOID VALVE (PART 2)
Check continuity between transmission unit harness connector terminal and ground.

Transmission unit harness connector | Ground | Continuity
Connector | Terminal
B49 | 14 | Ground | Not existed
15

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair or replace damaged parts.