REMOVAL

1.Remove the door finisher. Refer to Removal and Installation.

2.Disconnect the tweeter harness connector. Refer to Removal and Installation.

3.Remove the door corner cover inner. Refer to Exploded View.

4.Remove the corner piece mounting bolts (A), and then remove the corner piece (1) and the door inner seal (2).

5.Remove the sealing screen (1).
NOTE：
Cut butyl tape using a cutter knife so that tape remains on the sealing screen if the screen is reused.

6.Operate the power window switch to raise/lower the door glass until the glass bolts can be seen.
NOTE：
Connect the harness connector to the power window switch.

7.Loosen the door glass mounting bolt (A), and then remove the mounting bolt (B).

8.Pull the door glass (1) from the door panel while lifting it up over the door glass rear edge.

INSTALLATION
Install in the reverse order of removal.
NOTE：
Always perform the glass position adjustment.