1.PERFORM ECM SELF-DIAGNOSIS With CONSULT-III Perform self-diagnosis for “ENGINE”. Is any DTC detected? YES>>Check the DTC.
NO >>GO TO 2.
2.PERFORM SELF-DIAGNOSIS
With CONSULT-III

1. Erase self-diagnostic results for “ALL MODE AWD/4WD”.
2. Turn the ignition switch OFF.
3. Start the engine. Drive the vehicle for a while.
4. Make sure that malfunction indicator lamp (MIL) turns OFF.
5. Stop the vehicle. Perform self-diagnosis for “ALL MODE AWD/4WD”.

Is DTC “C1210” detected?
YES>> Replace AWD control unit. Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Check AWD control unit pin terminals for damage or loose connection with harness connector. If any items are damaged, repair or replace damaged parts.