REMOVAL

1.Remove air cleaner case and air duct assembly. Refer to Exploded View.

2.Disconnect turbocharger boost sensor harness connector.

3.Disconnect air inlet hose to remove the turbocharger boost sensor and the integrated recirculation valve and pipe.
NOTE：
Mark with paint for a reference purpose before removal.

4.Remove front bumper. Refer to Exploded View.

5.Remove air intake duct assembly. Refer to Exploded View (GT-R certified NISSAN dealer).

6.Disconnect air inlet hose and pipe to remove the charge air cooler assembly.
■ CAUTION ■
Never damage or scratch charge air cooler core when removing.

INSTALLATION
Note the following, and install in the reverse order of removal.
AIR INLET HOSE ASSEMBLY

A. | Matching mark (blue) | B. | Matching mark (yellow) | C. | Matching mark (pink)
| : Vehicle front |  |  |  |

- To install each part, refer to the above figure to align the matching marks.
- Temporarily assemble all the removed parts before tightening the clamp.
- Tighten the clamp to the specified torque as shown below:

  Clamp tightening torque | : 4.6 N·m (0.47 kg-m, 41 in-lb)

■ CAUTION ■
Never use air tool or power tools for tightening.
AIR INLET PIPE ASSEMBLY

- Install air inlet pipe assembly as follows:

1 | : Air inlet pipe assembly (bank 1)
2 | : Air inlet pipe assembly (bank 2)

1.Tighten bolt (A) (temporarily).

2.Tighten bolt (B) (temporarily).

3.Tighten bolt (C) (specified torque).

4.Tighten bolt (A) (specified torque).

5.Tighten bolt (B) (specified torque).