1.CHECK POWER STEERING PRESSURE SENSOR

1. Turn ignition switch OFF.
2. Reconnect all harness connectors disconnected.
3. Start engine and let it idle.
4. Check the voltage between ECM harness connector terminals under the following conditions.

   ECM | Condition | Voltage (V)
   Connector | + | –
   Terminal | Terminal
   F102 | 83 | 74 | Steering wheel | Being turned | 0.5 ‐ 4.5
   Not being turned | 0.4 ‐ 0.8

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace power steering pressure sensor.