Main “G” sensor generates signal voltage, when it detects deceleration beyond the specified level caused by vehicle frontal collision. OPERATION When air bag diagnosis sensor unit defines both signal voltage of the “G” sensor and the safing algorithm to be that of collision which exceeds a specified level, the driving circuit switches on and feeds the electric ignitor of both driver and passenger air bags and pre-tensioner seat belts.
STRUCTURE
Integrated type of the “G” sensor element for frontal collision with output terminals for signal voltage.
INSTALLATION
Crash zone sensor is installed on the radiator core support assembly with fixed nuts.