INSPECTION AFTER REMOVAL Wheel Hub and Bearing Assembly Check the wheel hub and bearing assembly for wear, cracks, and damage. Replace if necessary. Axle Housing Check the axle housing for wear, cracks, and damage. Replace if necessary.
Ball Joint Inspection
Check for boot breakage, axial looseness, and torque of suspension arm ball joint. Refer to Inspection (GT-R certified NISSAN dealer).
INSPECTION AFTER INSTALLATION

1.Adjust parking brake operation (stroke). Refer to Inspection and Adjustment.

2.Check wheel alignment. Refer to Inspection.

3.Adjust neutral position of steering angle sensor. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).