REMOVAL

1.Remove the trunk lid assembly. Refer to Removal and Installation.

2.Remove the trunk lid stay. Refer to Removal and Installation.

3.Remove the trunk lid hinge mounting bolts (body side), and then remove the trunk lid hinge.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Apply anticorrosive agent onto the mounting surface.
- Check trunk lid hinge rotating part for poor lubrication. If necessary, apply body grease.
- After installation, check trunk lid open/close, lock/unlock operation.
- After installation, perform the fitting adjustment. Refer to Adjustment.
- After installation, apply touch-up paint (the body color) onto the head of trunk lid hinge mounting bolts and nuts.