FLUID LEVEL

1.Check fluid level with engine stopped.

2.Check that fluid level is between MIN and MAX.
■ CAUTION ■
Adjust the fluid level to the R level (B) rather than the fluid level (A) in sports driving mode or in high road driving mode.

3.Fluid levels at HOT and COLD are different. Do not confuse them.

HOT | : Fluid temperature 50 – 80°C (122 – 176°F)
COLD | : Fluid temperature 0 – 30°C (32 – 86°F)

Recommended fluid | : Refer to Fluids and Lubricants.
Fluid capacity | : Refer to General Specifications.

■ CAUTION ■

- The fluid level must not exceed the MAX line. Excessive fluid causes fluid leakage from the cap.
- Never reuse drained power steering fluid.

FLUID LEAKAGE
Check hydraulic connections for fluid leakage, cracks, damage, looseness, or wear.

1.Run the engine until the fluid temperature reaches 50 to 80°C (122 to 176°F) in reservoir tank, and keep engine speed idle.

2.Turn steering wheel several times from full left stop to full right stop.

3.Hold steering wheel at each lock position for five seconds and carefully check for fluid leakage.
■ CAUTION ■
Never hold the steering wheel in a locked position for more than 10 seconds. (There is the possibility that power steering oil pump assembly may be damaged.)

4.If fluid leakage at connections occurs, loosen flare nut and then retighten. Do not overtighten connector as this can damage O-ring, washer and connector.

5.If fluid leakage from oil pump occurs, check oil pump. Refer to Inspection (GT-R certified NISSAN dealer).

6.Check steering gear boots for accumulation of fluid leakage from steering gear.