DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0882 | TCM power input signal low | A DTC is set if the power voltage input to TCM is less than 10.5 V. |

- Battery voltage drop
- TCM relay
- Harness or connector
  (Open in the power supply circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine and run at idle for 5 seconds or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine and run at idle for 5 seconds or more.
2. Check self-diagnosis.

Is DTC P0882 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.